Note that after the update, read the frequency first, then click this button to reset all the columns to the state where both R+T and receiving are allowed, and then write the frequency back. Otherwise, all channels will be prohibited from transmitting.

